













































































TLD DNS port is 53

Can you send multiple DNS questions and get multiple RR answers in one message? Yes

RTT0 + 2RTT(HTTP)

RTT0 + 5(2RTT(HTTP)) (1 OF THE 5 IS THE ESTABLISHING CONNECTION)

If the resource is updated, the ETag will change